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Abstract
Energy . In the current era of excessive energy consumption, production rates of energy are becoming inconsistent with communal demands.  Furthermore, the majority of contemporary methods used to produce energy are non-renewable, meaning that they cannot be readily replaced. In addition to this, energy sources such as fossil fuels are a prominent contributor to global pollution, ultimately leading to climate change. As an alternative to such harmful sources of energy, microalgal lipids can be used to artificially synthesize biodiesel which can, in turn, be used as a source of energy itself. To boost the yield of lipids extracted from microalgae, numerous chemical, mechanical and enzymatic pre-treatments methods can be employed. This investigation evaluates two widely used pre-treatment methods; osmotic shock (chemical) and thermal heating (mechanical); to determine their effectiveness and feasibility in industrial environments. Based on results from scientific experiments, thermal pre-treatment proved to be the most effective at increasing the yield of lipids. Although, while microwave pre-treatment is more effective, it also consumes significantly higher amounts of energy to apply. Consequently, posing osmotic shock as the more feasible and effective method. The findings of this research will assist industrialists and chemical engineering in selecting the most applicable pre-treatment method in the process of extracting lipids from microalgae.
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Fossil fuels are still the primary source of energy in Australia (fig 1.1). The rapid increase in global warming and immediate demand for energy has catalysed the search for an alternate means of energy production, specifically, renewable energy resources. 
Figure 1.1: Electricity Generation Across Australia. Retrieved from (Origin Energy, 2018)


[bookmark: _Toc51615779]Biodiesel
Among other renewable energy resources, biodiesel is a promising alternative to fossil fuels since it can directly be used in cars with diesel engines. However, a study shows that biodiesel when compared to Petro diesel increases fuel consumption by up to 11%. Regardless of this, biodiesel still produces 78% less carbon dioxide than conventional diesel fuel (Buyukkaya, 2010; National Renewable Energy Laboratory [NREL], 2005). In addition to this, it can be synthesised from lipids (hydrocarbons composed of fats and oils) obtained from plant materials (fig 1.2.), hence making it a renewable energy source. 



	 
Figure 1.2: Schematic of Biodiesel Production Path. Retrieved from (Alternate Fuels Data Centre, n.d.)


As stated by the U.S Department of Energy, approximately 100 pounds (45 kg) of biodiesel can be produced by appropriately reacting 100 pounds (45 kg) of oils and fats with 10 pounds (4.5 kg) of a short-chain alcohol. In addition to biodiesel, only one co-product is produced, glycerine, a type of sugar that is used in pharmaceutical and cosmetic products ("Alternative Fuels Data Centre: Biodiesel Production and Distribution", n.d.). 

[bookmark: _Toc51615780]Choice of Plant Material - Microalgae (Chlorella vulgaris)
In comparison to various plants, microalgae are  preferred due to its high lipid content per dry weight, swift growth rate and minimalistic land area requirement (He, 2016; Mata et al, 2009; Ramkumar & Kirubakaran, 2016). Chlorella vulgaris was chosen as the microalgae culture for this study since it was readily available in school (Lavars, 2019). Moreover, Chlorella vulgaris has the highest carbon dioxide sequestration rates among any other organic plant at around 0.1 - 0.7 g/litre/day (Lavars, 2019).
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Conventionally, lipids are extracted through the use of organic solvents. Common extraction methods include Floch method, Bligh & Dyer method and the Soxhlet technique (Kumar et al., 2015; Uduman et al., 2010). However, these methods pose a dangerous threat to the environment and humans due to the use of hazardous solvents and high energy consumption (Taher et al., 2014). Recently, researchers have found a novel approach to extract lipids from microalgae through the use of supercritical carbon dioxide (SC-CO2). Unlike the previously mentioned methods, SC-CO2 is an inert, nontoxic and an inexpensive fluid hence proving to be a better alternative in large scale industrial productions. However, due to limitations in the availability of equipment at school, organic solvent extraction was opted for this research. This does not affect the outcome of this study as the primary extraction method is a controlled variable.
[bookmark: _Toc51615782]Methods of Pre-treatment
Regardless of the primary extraction method used, there are a few problems associated with direct lipid extraction from microalgae, one being the relatively low yield of lipids. To solve this issue, scientists have found that pre-treating microalgae before extraction can potentially increase the amount of lipids obtained. By pre-treating microalgae, cell lysis occurs (disintegration of a cell by the rupture of the cell wall or membrane) which exposes the cytoplasm (a constituent within the cell that contains lipids and other essentials to protect it from being damaged). Following this procedure, solvents can be introduced to dissolve exposed lipids in the aqueous phase. 
Figure 1.3: Effect of Pre-treatment. Retrieved from (Angles, Jaouen, Pruvost & Marchal, 2017)




The process of which can be visualised by following figure 1.3, where on the left is an intact cell matrix containing lipids (yellow circles), that is subjected to a particular type of pre-treatment. As a result, the cell disintegrates, consequently releasing its contents (middle). After which, an organic solvent can be introduced to dissolve lipids present in the cell (right). 

All pre-treatment methods can be classified as mechanical or non-mechanical. Whereby, non-mechanical can further be subdivided into chemical and enzymatic. Figure 1.4 displays some of the concurrent methods used in a laboratory and/or industrial environment. [image: A screenshot of a cell phone

Description automatically generated] 
Figure 1.4: Types of Pre-treatment Methods. Retrieved from (Patel, Mikes & Matsakas, 2018)


Thermal pre-treatment subjects microalgal cells to microwaves for rapid heating which increases the internal temperature.  Therefore, the pressure gradient acting on the cell wall enhances mass transfer rates without lipid degradation (Uquiche et al., 2008). Alternatively, ‘osmotic shock’ is also equally advantageous where the abrupt exposure to lower osmotic pressure than in the cells, forces water to enter the cell structure. This increases the internal cell pressure causing cell lysis (Stanbury et al., 2017). 
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	Although there is a whole range of pre-treatments, very few studies compare the effects of chemical and mechanical pre-treatments. Furthermore, industrial compatibilities of each pre-treatment have not yet been properly evaluated in terms of the total energy applied to the system and the total amount of energy released in return, which is an important aspect to be considered when being used at an industrial scale. Moreover, the effects of pre-treatments and its efficiency vary depending on the specific microalgae culture implemented upon. 

[bookmark: _Toc51615784]Aim, Hypothesis & Variables in Research
	This study aims to provide an insight into two main pre-treatment methods under chemical and mechanical: osmotic-shock (chemical) and thermal/microwave-assisted (mechanical). In addition to this, part of this research is to also investigate the ease of application and industrial implication of each pre-treatment method. 

Hypothesis:
There will be no significant difference in the wt.% of lipids extracted between each of the two pre-treatments: osmotic shock and thermal heating. Although each method utilises a different scientific phenomenon, ultimately, both should disintegrate the cell structure. Hence, there should only be a negligible amount of difference in wt.% of lipids extracted due to natural differences in the amount of lipids present in each cell.

	Independent Variable
	Dependent Variable
	Controlled Variable

	· Pre-treatment Used
	· Lipid yield (wt.%)
· FAME contents
	· Type of microalgae
· Primary extraction Method


Variables to be Considered:
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The method used to conduct this research is a quantitative scientific experiment. Part of the scientific experiment was conducted in school laboratories under the supervision of trained laboratory technicians. Once the lipids were extracted, they were transferred to the Monash onsite campus situated in Clayton, where they were further analysed qualitatively and quantitatively using gas chromatography coupled with mass spectra analysis (GC-MS).

Three distinct sets of experiments will be carried out:
· Thermal (microwave) pretreatment before solvent-based extraction
· Osmotic Shock pretreatment before solvent-based extraction
· Organic Solvent extraction (controlled) without any pretreatment

2.1 Isolation and Preparation of Microalgae Culture
 Vials of microalgae dissolved in the growth media were collected and were centrifuged at 4500 rpm for five minutes. Following this, the growth media was deleted and the remaining contents in the vial were homogenised (the process of attaining uniformity throughout the solution). Subsequently, the contents in all of the vials were filtered using a standard Büchner funnel, with a filter paper of pore size: 7 micrometres. This was carried out to remove residual traces of microalgae growth media. Once thoroughly filtered, the filter paper, carrying the microalgae culture, was placed in a desiccator for one day, to evaporate water.
2.2 Thermal heating (Microwaves)
This procedure was performed using a classical microwave oven. The power output of the microwave was fixed at 1000W with a frequency of 2450 MHz. Upon completion, these can be compared against the increase in the percentage of lipids extracted using a bar chart to reveal the effects of various power outputs. 100 ± 0.05g of pre-dried microalgae was weighed using a balance and was set in a Pyrex bowl. It was then placed into the microwave oven and was treated over six cycles: samples were placed in a microwave for 1 min and were then allowed to be cooled to 25 ℃ (temperature was tracked using an infrared temperature gun), to ensure that the cells did not completely disintegrate (Dejoye et al., 2011).




	After harvesting microalgae from the growth media through centrifugation, the sample was added to a 500 ml shot bottle containing 200 ml pure deionised water and was left to rest until the salt concentration within deionised water was constant. The concentration of salt within the solution was measured using a LAQUA twin compact conductivity meter as shown in figure 2.1. A total of ten measurements were recorded over a span of 40 minutes with a gradual increase in the time difference (summarised in figure 2.2). Once the measured concentration was approximately constant, lipid extraction was immediately executed to prevent lipase proteins from breaking down exposed lipids. 

Figure 2.1: Conductivity Meter[image: A picture containing indoor, sitting, table, counter
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· Figure 2.2: Salinity measurements[image: A picture containing bus, group
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0. Method of Analysis
The extracts were analysed using gas chromatography since it offers high sensitivity and mainly because it can provide qualitative and quantitative insight into the composition of the lipid extract. The required apparatus for gas chromatography was provided by the Monash faculty. The column used was Helium and iso-octane was used as the primary carrier gas at a flow rate of 36 cm/s, split ratio 1:20, injector and detector temperature was set to 250 ℃. The oven temperature was programmed to 50 ℃ during the first minute, then was increased to 150 ℃ at a rate 10 ℃/min, and from 150 ℃ to 230 ℃ at a rate of 3 ℃/min, 5 min isothermal (held at constant temperature), then from 230 ℃ to 240 ℃ at a rate of 20 ℃/min and finally 10 minutes isothermal. Mass spectra were then acquired in m/z range 50-360 (Dejoye et al., 2011). The contents of the lipid extract were then identified by comparing their mass spectra using the NIST (National Institute of Standards and Technology) libraries and were also quantified by comparing the peak areas of known quantities. This information was then simplified for non-specialized public and was represented using a bar chart accompanied by a table to display the different constituents in the lipid extract and the quantity in which they were present.
0. Ethics
The microalgae culture used in this study: Chlorella vulgaris is not a pathogenic species. In other words, it poses no threat to human beings. A risk assessment was also conducted on ‘Student RiskAssess’ to evaluate any dangers in the experiments conducted. This experiment was rated at medium risk, for which extra precautionary measures were taken, such as, using appropriate safety apparatus and watching demonstrations on the handling procedures of Hexane and Methanol. 

On the other hand, a serious ethical concern is that a new battle may emerge for land usage between food and fuel. This is because land is a finite resource and once it's used to cultivate microalgae it cannot, at a later stage, be used to grow crops. However, this can be potentially mitigated, since microalgae can also be grown in wastewater land. Although, more research must be done to test the effects of doing so. 
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