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Split ring commutator reverses current every half
turn to swap direction of force and maintain
continuous torque in one direction.
e current reverses every half cycle.
e when current reverses, so do the directions of
the force couple.
e the loop’s momentum will carry it into a
position where the reversed forces will cont. the
rotation.
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Orbital Radius = Planet Radius + Altitude.
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3 ways to increase the strength of the magnetic field of a solenoid
- Use a ferro-magnetic core|
- Increase the current through the solenoid
- Increase the number of turns around the iron core
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- Change the direction of current every half turn

- Changes the direction of force every half turn on the side (context)
- Maintains the direction of torque in the coil in (context) direction.
- Maintains electrical contact without tangling during rotation




